DETAILS

MEIKO TOPCLEAN D SCBA AND PPE EQUIPMENT WASHER

TopClean D cleans and decontaminates a wide range of equipment – from SCBA to tanks, masks, helmets, boots and other PPE.

**MEIKO’s ActivePlus**wash-water filter system creates the cleanest water possible by filtering tank water multiple times throughout the wash. Dirt, grime and  toxins are washed out when the filter is backflushed at specific intervals.

**Auto Safe**temperature control ensures a final rinse temperature of 120°F (49°C) regardless of the incoming water temperature (hot-water supply preferred).

**Technology** that gives you operating control and convenience. Meet MIKE 2, the fully electronic control system from MEIKO. It’s standard on DECON Series equipment washers. Choose from DECON’s three wash programs with one touch on the keypad.

**Soft Start** slowly engages the wash pump and gradually builds water pressure to help prevent PPE from moving on the rack.

**Aqua Stop,** MEIKO’s built-in leak detection system, turns off the external fill valve if an internal leak is detected, and also provides troubleshooting messages to the operator.

**Built-in booster heater** with power rinse pump ensures final rinse pressure and temperature, for consistent, high-quality cleaning results.

**Features**

* 20 cycles per hour using just 2.37 gallons (8.97 liters) of water per cycle.
* Variable program cycles for varying soil levels: 3 minutes, 8 minutes, and 8+ minutes (includes an automatic water change for heavily soiled items).
* Double-wall construction provides extra insulation, keeps heat inside the machine so it’s cool to the
* touch, conserves energy and reduces noise for a quieter environment.
* Corrosion-resistant 304 and 316L stainless steel construction.
* Stainless steel non-clogging wash and rinse arms.
* Type A air gap system.
* Machine shutdown automatically initiates a rinse cycle for the entire wash chamber to help
* make cleaning easier.
* Custom stainless steel basket with mask holder inserts.
* Oscillating wash arms provide complete coverage of gear - even in the corners!
* Built-in, fully automatic liquid detergent and rinse-aid pumps.
* Powerful 3½ hp (2.6 kW) wash pump. Pumped drain for floor and wall drain applications.
* Fully automatic fill, start, dump and refill, as well as automatic reset.